**MAGNETIC LEVER SWITCH**

The reed switch is contained within a large hinged case with the switch on one lid and its balancing magnet on the other lid. Opening the case by approximately 1 in (2.5m) with the fingers, raises the alarm as the reed switch opens. The switch is normally armed in the closed position.

Advantage ;

* Almost totally silent operation

Disadvantage :

* They require someone to operate the lid